TITLE: New CNUT package for 8.2.1
 
PRODUCTS:  Canopy PTP and PTMP Radios
 
RELEASE: 8.2.1
 
PROBLEM DESCRIPTION:  Auto-update fails to update radios when using an external TFTP server.  In addition we are seeing instances where CNUT or Prizm may report that BH radios fail to upgrade but actually do complete the upgrade process.


SOFTWARE REQUIRED FOR WORK AROUND:  
Download new R8.2.1 CNUT package (“CANOPY_8.2.1_DES_V2.zip” or “CANOPY_8.2.1_AES_V2.zip” for AES modules) from http://motorola.canopywireless.com/support/software

Note: The software itself has not changed, only the CNUT pkg2 file.

Radios already upgraded with the previous R8.2.1 CNUT package (“CANOPY_8.2.1_DES.zip” or “CANOPY_8.2.1_AES.zip” for AES modules) do not need upgrading with the new R8.2.1 package.

IMPORTANT: It is recommended to remove previous R8.2.1 package from CNUT or PRIZM and replace them with the new R8.2.1 CNUT package


POINT OF CONTACT FOR WORK AROUND SOFTWARE (If required):  Please contact Canopy support at technical-support@canopywireless.com


KEYWORDS:  auto-update, 8.2.1, BH, CNUT, timeout, package

 
