--
-- 	whisp-reg.mib
--
--      *************************************************************************************
--	Copyright 2003 (c) , Motorola, Inc.
--      Motorola Confidential Proprietary
--      *************************************************************************************
--
--	This module contains registrations for Canopy related items such
--	as the identity of products, product components and other MIB
--	related items.
--      
--      *************************************************************************************
--	$Id: WHISP-GLOBAL-REG-MIB.txt,v 1.2 2006/11/22 17:26:04 y17557 Exp $
--
--      Revision History:
--
--      <Date>                  <Author>                <Changes>
--      01/31/2002                Y.G              	Initial release.
--      08/24/2005                M.D              	Change OS type for ucos.
--		05/02/2006				  M.D				Add new global OID definitions
--		07/12/2006		  		  V.G				Add new global OIDs whispPlvModem and whispPlvGateway
--		11/10/2006		  		  V.G				Add new global OID whispPlvRepeater and
--                                                  whispPlvBridge
--      **************************************************************************************

WHISP-GLOBAL-REG-MIB DEFINITIONS ::= BEGIN
IMPORTS
	MODULE-IDENTITY,
	enterprises
		FROM SNMPv2-SMI;

whispGlobalRegModule 	MODULE-IDENTITY
	LAST-UPDATED	"200304100000Z"
	ORGANIZATION	"Motorola"
	CONTACT-INFO
		"Canopy Technical Support
		email: technical-support@canopywireless.com"
	DESCRIPTION
		"The Canopy central registration module."
	::= {whispModules 1}

-- the root of the sub-tree for Canopy Radio Modem Product Line.
mot		OBJECT IDENTIFIER ::= {enterprises 161}
whispRoot	OBJECT IDENTIFIER ::= {mot 19}

-- sub-tree for registrations, which includes modules
whispReg	OBJECT IDENTIFIER ::= {whispRoot 1}

-- sub-tree for WHiSP wide objects and events
whispGeneric	OBJECT IDENTIFIER ::= {whispRoot 2}

-- sub-tree for WHiSP product specific objects and events
whispProducts	OBJECT IDENTIFIER ::= {whispRoot 3}

--      Product registrations. The OIDs should be assigned to
--      sysObjectID of the system group in SNMPv2-MIB supported
--      by the agent. A manager needs to know the (unique) IP 
--      address of the agent and get the value (OID value) of
--      sysObjectID to uniquely identify the agent type. Once the
--      agent type has been identified, the manager will know what
--      MIBs the agent supports (from agent capabilities).

        whispAps        OBJECT IDENTIFIER ::= {whispProducts 1}
        whispSm         OBJECT IDENTIFIER ::= {whispProducts 2}
        whispBox        OBJECT IDENTIFIER ::= {whispProducts 3}
        whispCMM        OBJECT IDENTIFIER ::= {whispProducts 4}
		whispPlv        OBJECT IDENTIFIER ::= {whispProducts 5}
		whispCMM4       OBJECT IDENTIFIER ::= {whispProducts 6}
        whispPlvModem   OBJECT IDENTIFIER ::= {whispProducts 7}
		whispPlvGateway OBJECT IDENTIFIER ::= {whispProducts 8}
		whispPlvRepeater OBJECT IDENTIFIER ::= {whispProducts 9}
        whispPlvBridge   OBJECT IDENTIFIER ::= {whispProducts 10}
       
-- the Canopy modules registrations
        whispModules OBJECT IDENTIFIER ::= {whispReg 1}

-- These are the returned values of the agent type.
-- returned to:  .iso.org.dod.internet.mgmt.mib-2.system.sysObjectID.0 

--SNMP agent for Canopy units
canopySnmpAgent      OBJECT IDENTIFIER ::= { whispRoot 250 }

--Canopy SNMP agent OID definition
ucos           OBJECT IDENTIFIER ::= { canopySnmpAgent 256 }

-- prizm snmp agent 
prizmSnmpAgent	OBJECT IDENTIFIER ::= { whispRoot 1250 }

-- prizm managed object subtree
prizm	OBJECT IDENTIFIER ::= {whispRoot 1000}

END
